Data Flow Diagram – Manufacturing Quality

Completed product

Faulty product,

Send to further inspect

No

Repeat the sensor

data review process

for all sensors –

in this case 589 times

Yes

Send product down manufacture line

Review sensor data

Meet quality: Yes/No

Collect data from sensor

Manufacture belt/machine

Raw materials